**INSTRUCTION LivelyForm** December 2012

***Make sure everything is connected:***

1. **Plugin the design to the box**
2. **Plugin Box to 24 V and 5V power supply  
   Turn on the box => then red LED on box should light red**

***Before Interaction:***

1. **Use the RED buttons   
   to set the maximal closed position**(in between a U-shape and a closed circle,)
2. **Turn potentiometer clockwise to minimum sensitivity**
3. **Press the green button   
   => then the LED will turn green and LF will start opening and lighting.**

***Calibration:***

1. **Touch one of the sections and check that it moves a little and then stops**
   1. **If it does not move when touching a section and all leds are green:**
      1. **Then increase the LF touch-sensitivity by turning the potentiometer counter-clockwise a little until it moves and stops.**
         * **the leds have to run yellow from center to outwards**
   2. **If it does moves, but does not stop when touching a single section and leds do not run all the way from center to outwards.**
      1. **Then decrease the LF touch-sensitivity by turning the potentiometer clockwise a little until it stops moving**
         * **The leds have to run yellow from center to outwards.**
2. **Repeat for each of the sections**

(very sensitive, so be patient)

1. **Ready to use**

***While in use:***

1. **If it does not respond to touch and all leds are glowing green, then increase sensitivity by turning the potentiometer counter-clockwise until it starts moving when touched.**
2. **If it moves by itself without being touched, then decrease sensitivity by turning the potentiometer clockwise until it stops moving and all leds glow green**
3. **If during interaction it starts opening all the way. Turn off the design from the box switch immediately!!!**