**INSTRUCTION LivelyForm** October 2011

**ALWAYS UNPLUG AFTER USE**

1. **Plugin the design to the box**
2. **Plug in Power plug number 1   
   before number 2  
   => then red LED on box should light   
    & the design should light up (at least when touched)**

***On the box:***

1. **Use the RED buttons   
   to set the maximal closed position**(in between a U-shape and a closed circle,)
2. **Press the green button   
   => then the LED will turn green**
3. **Calibrate the designs touch-sensitivity   
   by turning the potentiometer  
     
   so it only just starts to close when touched**(very sensitive, so be patient)
4. **Ready to use**

***If no red light try*: Turn ON.. wait 5 sec…Turn OFF&ON fast**

**ALWAYS UNPLUG AFTER USE**

**INSTRUKTION LivelyForm** Oktober 2011

**TRÆK ALTID STIKKENE UD EFTER BRUG  
efterlad ikke designets stik i kontakten**

1. **Sæt designet i kassens stik**
2. **Sæt de 2 el-stik nummer 1 i kontakten   
    Derefter stik nummer 2  
   => rød LED-lys på kassen bør lyse & designet bør lyse**

***På kassen:***

1. **Tryk på de røde trykknapper på kassen  
   til at stille designets mest lukkede position**(mellem et U og en cirkle)
2. **Tryk på den grønne tryk knap   
   => så bør LED-lyset på kassen lyse grønt**
3. **Indstil drejeknappen på kassen,   
   således at designet kun lige præcist   
   begynder at lukke sig når man rør**(finindstilling for hver gang, det er ikke helt let)  
    NB det er det nærmeste der påvirker   
    så når I indstiller så sid lidt væk
4. **PARAT !**

***Hvis det ikke fungerer:*  
Tænd (I) ON … vent så 5 sekunder … Tænd(I)-Sluk(O) hurtigt**

**TRÆK ALTID STIKKENE UD EFTER BRUG**